A B C D E F G H I L M N O P R S T U V W

## B

B_FastSerial - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Hardware Option - Interface B Fast Serial
B_FastSerial - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Hardware Option - Interface B Fast Serial
B_FIFO - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Hardware Option - Interface B 245 FIFO
B_FIFO - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Hardware Option - Interface B 245 FIFO
B_FIFOTarget - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Hardware Option - Interface B 245 FIFO CPU Target
B_FIFOTarget - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Hardware Option - Interface B 245 FIFO CPU Target
B_HighIO - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Drive Option - Interface B High Current IO
B_LoadD2XX - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Driver Option - Interface B Load D2XX
B_LoadD2XX - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Driver Option - Interface B Load D2XX Port
B_LoadVCP - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Driver Option - Interface B Load Vitrual Com Port
B_LoadVCP - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Driver Option - Interface B Load virtual Com Port
B_UART - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Drive Option - Interface B UART
B_UART - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Hardware Option - Interface B 245 UART
bcdDevice - Variable in class com.ftdi.j2xx.D2xxManager.FtDeviceInfoListNode
  Indicate USB specification release number(BCD).
BCDDisableSleep - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Battery Charge Detect option - Disable Sleep
BCDEnable - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Battery Charge Detect option - Enable
BCDForceCBusPWREN - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Battery Charge Detect option - Force CBus Power Enable
BH_DriveCurrent - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Drive Option - BH pins have driver current.
BH_DriveCurrent - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Drive Option - BH pins drive current.
BH_LoadD2XX - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Driver Option - Interface BH Load D2XX
BH_LoadRI_RS485 - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Driver Option - Interface BH Load RI_RS485
BH_LoadVCP - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Driver Option - Interface BH Load Vitrual Com Port
BH_RI_TXDEN - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Hardware Option - Interface BH uses RI as RS485 TXDEN
BH_SchmittInput - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Drive Option - BH pins have schmitt input.
BH_SchmittInput - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Drive Option - BH pins have Schmitt input.
BH_SlowSlew - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Drive Option - BH pins have slow slew.
BH_SlowSlew - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Drive Option - BH pins have slow slew.
BL_DriveCurrent - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Drive Option - BL pins have driver current.
BL_DriveCurrent - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Drive Option - BL pins drive current.
BL_DriveCurrent - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Drive Option - BL pins Drive Current.
BL_LoadD2XX - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Driver Option - Interface BL Load D2XX
BL_LoadRI_RS485 - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Driver Option - Interface BL Load RI_RS485
BL_LoadVCP - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Driver Option - Interface BL Load Vitrual Com Port
BL_RI_TXDEN - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Hardware Option - Interface BL uses RI as RS485 TXDEN
BL_SchmittInput - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Drive Option - BL pins have schmitt input.
BL_SchmittInput - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Drive Option - BL pins have Schmitt input.
BL_SchmittInput - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Drive Option - BL pins have Schmitt input.
BL_SlowSlew - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Drive Option - BL pins have slow slew.
BL_SlowSlew - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Drive Option - BL pins have slow slew.
BL_SlowSlew - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Drive Option - BL pins have slow slew.
breakOnParam - Variable in class com.ftdi.j2xx.D2xxManager.FtDeviceInfoListNode
  Indicate breakOnParam variable to representation UART break status Default value is 0x0008; Device can set break on via `FT_Device.setBreakOn()` method.

A B C D E F G H I L M N O P R S T U V W

About FTDI | FTDI Licence Terms