A B C D E F G H I L M N O P R S T U V W

## P

PowerSaveEnable - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Hardware Option - Power Save Enable if using BCBus7 to save power for self-powered designs.
PowerSaveEnable - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - Power Save Enable if using BCBus7 to save power for self-powered designs.
PowerSaveEnable - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - Power Save Enable if using BCBus7 to save power for self-powered designs.
Product - Variable in class com.ftdi.j2xx.FT_EEPROM
  String Descriptor - Product String
ProductId - Variable in class com.ftdi.j2xx.FT_EEPROM
  Device Descriptor - Product ID
PullDownEnable - Variable in class com.ftdi.j2xx.FT_EEPROM
  Hardware Option - Pull Down In Suspend Enabled
purge(byte) - Method in class com.ftdi.j2xx.FT_Device
  Discards any data form the specified driver buffer and also flushes data from the device.

A B C D E F G H I L M N O P R S T U V W

About FTDI | FTDI Licence Terms